>CB          CB
>ED          ED
>DD          DD
>FD          FD
>DDCB        DDCB
>FDCB        FDCB
>00          NOP
>01          LD BC,nn
>02          LD (BC),A
>03          INC BC
>04          INC B
>05          DEC B
>06          LD B,n
>07          RLCA
>08          EX AF,AF’
>09          ADD HL,BC
>0A          LD A,(BC)
>0B          DEC BC
>0C          INC C
>0D          DEC C
>0E          LD C,n
>0F          RRCA
>10          DJNZ (PC+e)
>11          LD DE,nn
>12          LD (DE),A
>13          INC DE
>14          INC D
>15          DEC D
>16          LD D,n
>17          RLA
>18          JR (PC+e)
>19          ADD HL,DE
>1A          LD A,(DE)
>1B          DEC DE
>1C          INC E
>1D          DEC E
>1E          LD E,n
>1F          RRA
>20          JR NZ,(PC+e)
>21          LD HL,nn
>22          LD (nn),HL
>23          INC HL
>24          INC H
>25          DEC H
>26          LD H,n
>27          DAA
>28          JR Z,(PC+e)
>29          ADD HL,HL
>2A          LD HL,(nn)
>2B          DEC HL
>2C          INC L
>2D          DEC L
>2E          LD L,n
>2F          CPL
>30          JR NC,(PC+e)
>31          LD SP,nn
>32          LD (nn),A
>33          INC SP
>34          INC (HL)
>35          DEC (HL)
>36          LD (HL),n
>37          SCF
>38          JR C,(PC+e)
>39          ADD HL,SP
>3A          LD A,(nn)
>3B          DEC SP
>3C          INC A
>3D          DEC A
>3E          LD A,n
>3F          CCF
>40          LD B,B
>41          LD B,C
>42          LD B,D
>43          LD B,E
>44          LD B,H
>45          LD B,L
>46          LD B,(HL)
>47          LD B,A
>48          LD C,B
>49          LD C,C
>4A          LD C,D
>4B          LD C,E
>4C          LD C,H
>4D          LD C,L
>4E          LD C,(HL)
>4F          LD C,A
>50          LD D,B
>51          LD D,C
>52          LD D,D
>53          LD D,E
>54          LD D,H
>55          LD D,L
>56          LD D,(HL)
>57          LD D,A
>58          LD E,B
>59          LD E,C
>5A          LD E,D
>5B          LD E,E
>5C          LD E,H
>5D          LD E,L
>5E          LD E,(HL)
>5F          LD E,A
>60          LD H,B
>61          LD H,C
>62          LD H,D
>63          LD H,E
>64          LD H,H
>65          LD H,L
>66          LD H,(HL)
>67          LD H,A
>68          LD L,B
>69          LD L,C
>6A          LD L,D
>6B          LD L,E
>6C          LD L,H
>6D          LD L,L
>6E          LD L,(HL)
>6F          LD L,A
>70          LD (HL),B
>71          LD (HL),C
>72          LD (HL),D
>73          LD (HL),E
>74          LD (HL),H
>75          LD (HL),L
>76          HALT
>77          LD (HL),A
>78          LD A,B
>79          LD A,C
>7A          LD A,D
>7B          LD A,E
>7C          LD A,H
>7D          LD A,L
>7E          LD A,(HL)
>7F          LD A,A
>80          ADD A,B
>81          ADD A,C
>82          ADD A,D
>83          ADD A,E
>84          ADD A,H
>85          ADD A,L
>86          ADD A,(HL)
>87          ADD A,A
>88          ADC A,B
>89          ADC A,C
>8A          ADC A,D
>8B          ADC A,E
>8C          ADC A,H
>8D          ADC A,L
>8E          ADC A,(HL)
>8F          ADC A,A
>90          SUB B
>91          SUB C
>92          SUB D
>93          SUB E
>94          SUB H
>95          SUB L
>96          SUB (HL)
>97          SUB A
>98          SBC A,B
>99          SBC A,C
>9A          SBC A,D
>9B          SBC A,E
>9C          SBC A,H
>9D          SBC A,L
>9E          SBC A,(HL)
>9F          SBC A,A
>A0          AND B
>A1          AND C
>A2          AND D
>A3          AND E
>A4          AND H
>A5          AND L
>A6          AND (HL)
>A7          AND A
>A8          XOR B
>A9          XOR C
>AA          XOR D
>AB          XOR E
>AC          XOR H
>AD          XOR L
>AE          XOR (HL)
>AF          XOR A
>B0          OR B
>B1          OR C
>B2          OR D
>B3          OR E
>B4          OR H
>B5          OR L
>B6          OR (HL)
>B7          OR A
>B8          CP B
>B9          CP C
>BA          CP D
>BB          CP E
>BC          CP H
>BD          CP L
>BE          CP (HL)
>BF          CP A
>C0          RET NZ
>C1          POP BC
>C2          JP NZ,nn
>C3          JP nn
>C4          CALL NZ,nn
>C5          PUSH BC
>C6          ADD A,n
>C7          RST 0H
>C8          RET Z
>C9          RET
>CA          JP Z,nn
>CB00        RLC B
>CB01        RLC C
>CB02        RLC D
>CB03        RLC E
>CB04        RLC H
>CB05        RLC L
>CB06        RLC (HL)
>CB07        RLC A
>CB08        RRC B
>CB09        RRC C
>CB0A        RRC D
>CB0B        RRC E
>CB0C        RRC H
>CB0D        RRC L
>CB0E        RRC (HL)
>CB0F        RRC A
>CB10        RL B
>CB11        RL C
>CB12        RL D
>CB13        RL E
>CB14        RL H
>CB15        RL L
>CB16        RL (HL)
>CB17        RL A
>CB18        RR B
>CB19        RR C
>CB1A        RR D
>CB1B        RR E
>CB1C        RR H
>CB1D        RR L
>CB1E        RR (HL)
>CB1F        RR A
>CB20        SLA B
>CB21        SLA C
>CB22        SLA D
>CB23        SLA E
>CB24        SLA H
>CB25        SLA L
>CB26        SLA (HL)
>CB27        SLA A
>CB28        SRA B
>CB29        SRA C
>CB2A        SRA D
>CB2B        SRA E
>CB2C        SRA H
>CB2D        SRA L
>CB2E        SRA (HL)
>CB2F        SRA A
>CB30        SLL B*
>CB31        SLL C*
>CB32        SLL D*
>CB33        SLL E*
>CB34        SLL H*
>CB35        SLL L*
>CB36        SLL (HL)*
>CB37        SLL A*
>CB38        SRL B
>CB39        SRL C
>CB3A        SRL D
>CB3B        SRL E
>CB3C        SRL H
>CB3D        SRL L
>CB3E        SRL (HL)
>CB3F        SRL A
>CB40        BIT 0,B
>CB41        BIT 0,C
>CB42        BIT 0,D
>CB43        BIT 0,E
>CB44        BIT 0,H
>CB45        BIT 0,L
>CB46        BIT 0,(HL)
>CB47        BIT 0,A
>CB48        BIT 1,B
>CB49        BIT 1,C
>CB4A        BIT 1,D
>CB4B        BIT 1,E
>CB4C        BIT 1,H
>CB4D        BIT 1,L
>CB4E        BIT 1,(HL)
>CB4F        BIT 1,A
>CB50        BIT 2,B
>CB51        BIT 2,C
>CB52        BIT 2,D
>CB53        BIT 2,E
>CB54        BIT 2,H
>CB55        BIT 2,L
>CB56        BIT 2,(HL)
>CB57        BIT 2,A
>CB58        BIT 3,B
>CB59        BIT 3,C
>CB5A        BIT 3,D
>CB5B        BIT 3,E
>CB5C        BIT 3,H
>CB5D        BIT 3,L
>CB5E        BIT 3,(HL)
>CB5F        BIT 3,A
>CB60        BIT 4,B
>CB61        BIT 4,C
>CB62        BIT 4,D
>CB63        BIT 4,E
>CB64        BIT 4,H
>CB65        BIT 4,L
>CB66        BIT 4,(HL)
>CB67        BIT 4,A
>CB68        BIT 5,B
>CB69        BIT 5,C
>CB6A        BIT 5,D
>CB6B        BIT 5,E
>CB6C        BIT 5,H
>CB6D        BIT 5,L
>CB6E        BIT 5,(HL)
>CB6F        BIT 5,A
>CB70        BIT 6,B
>CB71        BIT 6,C
>CB72        BIT 6,D
>CB73        BIT 6,E
>CB74        BIT 6,H
>CB75        BIT 6,L
>CB76        BIT 6,(HL)
>CB77        BIT 6,A
>CB78        BIT 7,B
>CB79        BIT 7,C
>CB7A        BIT 7,D
>CB7B        BIT 7,E
>CB7C        BIT 7,H
>CB7D        BIT 7,L
>CB7E        BIT 7,(HL)
>CB7F        BIT 7,A
>CB80        RES 0,B
>CB81        RES 0,C
>CB82        RES 0,D
>CB83        RES 0,E
>CB84        RES 0,H
>CB85        RES 0,L
>CB86        RES 0,(HL)
>CB87        RES 0,A
>CB88        RES 1,B
>CB89        RES 1,C
>CB8A        RES 1,D
>CB8B        RES 1,E
>CB8C        RES 1,H
>CB8D        RES 1,L
>CB8E        RES 1,(HL)
>CB8F        RES 1,A
>CB90        RES 2,B
>CB91        RES 2,C
>CB92        RES 2,D
>CB93        RES 2,E
>CB94        RES 2,H
>CB95        RES 2,L
>CB96        RES 2,(HL)
>CB97        RES 2,A
>CB98        RES 3,B
>CB99        RES 3,C
>CB9A        RES 3,D
>CB9B        RES 3,E
>CB9C        RES 3,H
>CB9D        RES 3,L
>CB9E        RES 3,(HL)
>CB9F        RES 3,A
>CBA0        RES 4,B
>CBA1        RES 4,C
>CBA2        RES 4,D
>CBA3        RES 4,E
>CBA4        RES 4,H
>CBA5        RES 4,L
>CBA6        RES 4,(HL)
>CBA7        RES 4,A
>CBA8        RES 5,B
>CBA9        RES 5,C
>CBAA        RES 5,D
>CBAB        RES 5,E
>CBAC        RES 5,H
>CBAD        RES 5,L
>CBAE        RES 5,(HL)
>CBAF        RES 5,A
>CBB0        RES 6,B
>CBB1        RES 6,C
>CBB2        RES 6,D
>CBB3        RES 6,E
>CBB4        RES 6,H
>CBB5        RES 6,L
>CBB6        RES 6,(HL)
>CBB7        RES 6,A
>CBB8        RES 7,B
>CBB9        RES 7,C
>CBBA        RES 7,D
>CBBB        RES 7,E
>CBBC        RES 7,H
>CBBD        RES 7,L
>CBBE        RES 7,(HL)
>CBBF        RES 7,A
>CBC0        SET 0,B
>CBC1        SET 0,C
>CBC2        SET 0,D
>CBC3        SET 0,E
>CBC4        SET 0,H
>CBC5        SET 0,L
>CBC6        SET 0,(HL)
>CBC7        SET 0,A
>CBC8        SET 1,B
>CBC9        SET 1,C
>CBCA        SET 1,D
>CBCB        SET 1,E
>CBCC        SET 1,H
>CBCD        SET 1,L
>CBCE        SET 1,(HL)
>CBCF        SET 1,A
>CBD0        SET 2,B
>CBD1        SET 2,C
>CBD2        SET 2,D
>CBD3        SET 2,E
>CBD4        SET 2,H
>CBD5        SET 2,L
>CBD6        SET 2,(HL)
>CBD7        SET 2,A
>CBD8        SET 3,B
>CBD9        SET 3,C
>CBDA        SET 3,D
>CBDB        SET 3,E
>CBDC        SET 3,H
>CBDD        SET 3,L
>CBDE        SET 3,(HL)
>CBDF        SET 3,A
>CBE0        SET 4,B
>CBE1        SET 4,C
>CBE2        SET 4,D
>CBE3        SET 4,E
>CBE4        SET 4,H
>CBE5        SET 4,L
>CBE6        SET 4,(HL)
>CBE7        SET 4,A
>CBE8        SET 5,B
>CBE9        SET 5,C
>CBEA        SET 5,D
>CBEB        SET 5,E
>CBEC        SET 5,H
>CBED        SET 5,L
>CBEE        SET 5,(HL)
>CBEF        SET 5,A
>CBF0        SET 6,B
>CBF1        SET 6,C
>CBF2        SET 6,D
>CBF3        SET 6,E
>CBF4        SET 6,H
>CBF5        SET 6,L
>CBF6        SET 6,(HL)
>CBF7        SET 6,A
>CBF8        SET 7,B
>CBF9        SET 7,C
>CBFA        SET 7,D
>CBFB        SET 7,E
>CBFC        SET 7,H
>CBFD        SET 7,L
>CBFE        SET 7,(HL)
>CBFF        SET 7,A
>CC          CALL Z,nn
>CD          CALL nn
>CE          ADC A,n
>CF          RST 8H
>D0          RET NC
>D1          POP DE
>D2          JP NC,nn
>D3          OUT (n),A
>D4          CALL NC,nn
>D5          PUSH DE
>D6          SUB n
>D7          RST 10H
>D8          RET C
>D9          EXX
>DA          JP C,nn
>DB          IN A,(n)
>DC          CALL C,nn
>DD09        ADD IX,BC
>DD19        ADD IX,DE
>DD21        LD IX,nn
>DD22        LD (nn),IX
>DD23        INC IX
>DD24        INC IXH*
>DD25        DEC IXH*
>DD26        LD IXH,n*
>DD29        ADD IX,IX
>DD2A        LD IX,(nn)
>DD2B        DEC IX
>DD2C        INC IXL*
>DD2D        DEC IXL*
>DD2E        LD IXL,n*
>DD34        INC (IX+d)
>DD35        DEC (IX+d)
>DD36        LD (IX+d),n
>DD39        ADD IX,SP
>DD44        LD B,IXH*
>DD45        LD B,IXL*
>DD46        LD B,(IX+d)
>DD4C        LD C,IXH*
>DD4D        LD C,IXL*
>DD4E        LD C,(IX+d)
>DD54        LD D,IXH*
>DD55        LD D,IXL*
>DD56        LD D,(IX+d)
>DD5C        LD E,IXH*
>DD5D        LD E,IXL*
>DD5E        LD E,(IX+d)
>DD60        LD IXH,B*
>DD61        LD IXH,C*
>DD62        LD IXH,D*
>DD63        LD IXH,E*
>DD64        LD IXH,IXH*
>DD65        LD IXH,IXL*
>DD66        LD H,(IX+d)
>DD67        LD IXH,A*
>DD68        LD IXL,B*
>DD69        LD IXL,C*
>DD6A        LD IXL,D*
>DD6B        LD IXL,E*
>DD6C        LD IXL,IXH*
>DD6D        LD IXL,IXL*
>DD6E        LD L,(IX+d)
>DD6F        LD IXL,A*
>DD70        LD (IX+d),B
>DD71        LD (IX+d),C
>DD72        LD (IX+d),D
>DD73        LD (IX+d),E
>DD74        LD (IX+d),H
>DD75        LD (IX+d),L
>DD77        LD (IX+d),A
>DD7C        LD A,IXH*
>DD7D        LD A,IXL*
>DD7E        LD A,(IX+d)
>DD84        ADD A,IXH*
>DD85        ADD A,IXL*
>DD86        ADD A,(IX+d)
>DD8C        ADC A,IXH*
>DD8D        ADC A,IXL*
>DD8E        ADC A,(IX+d)
>DD94        SUB IXH*
>DD95        SUB IXL*
>DD96        SUB (IX+d)
>DD9C        SBC A,IXH*
>DD9D        SBC A,IXL*
>DD9E        SBC A,(IX+d)
>DDA4        AND IXH*
>DDA5        AND IXL*
>DDA6        AND (IX+d)
>DDAC        XOR IXH*
>DDAD        XOR IXL*
>DDAE        XOR (IX+d)
>DDB4        OR IXH*
>DDB5        OR IXL*
>DDB6        OR (IX+d)
>DDBC        CP IXH*
>DDBD        CP IXL*
>DDBE        CP (IX+d)
>DDCB00      LD B,RLC (IX+d)*
>DDCB01      LD C,RLC (IX+d)*
>DDCB02      LD D,RLC (IX+d)*
>DDCB03      LD E,RLC (IX+d)*
>DDCB04      LD H,RLC (IX+d)*
>DDCB05      LD L,RLC (IX+d)*
>DDCB06      RLC (IX+d)
>DDCB07      LD A,RLC (IX+d)*
>DDCB08      LD B,RRC (IX+d)*
>DDCB09      LD C,RRC (IX+d)*
>DDCB0A      LD D,RRC (IX+d)*
>DDCB0B      LD E,RRC (IX+d)*
>DDCB0C      LD H,RRC (IX+d)*
>DDCB0D      LD L,RRC (IX+d)*
>DDCB0E      RRC (IX+d)
>DDCB0F      LD A,RRC (IX+d)*
>DDCB10      LD B,RL (IX+d)*
>DDCB11      LD C,RL (IX+d)*
>DDCB12      LD D,RL (IX+d)*
>DDCB13      LD E,RL (IX+d)*
>DDCB14      LD H,RL (IX+d)*
>DDCB15      LD L,RL (IX+d)*
>DDCB16      RL (IX+d)
>DDCB17      LD A,RL (IX+d)*
>DDCB18      LD B,RR (IX+d)*
>DDCB19      LD C,RR (IX+d)*
>DDCB1A      LD D,RR (IX+d)*
>DDCB1B      LD E,RR (IX+d)*
>DDCB1C      LD H,RR (IX+d)*
>DDCB1D      LD L,RR (IX+d)*
>DDCB1E      RR (IX+d)
>DDCB1F      LD A,RR (IX+d)*
>DDCB20      LD B,SLA (IX+d)*
>DDCB21      LD C,SLA (IX+d)*
>DDCB22      LD D,SLA (IX+d)*
>DDCB23      LD E,SLA (IX+d)*
>DDCB24      LD H,SLA (IX+d)*
>DDCB25      LD L,SLA (IX+d)*
>DDCB26      SLA (IX+d)
>DDCB27      LD A,SLA (IX+d)*
>DDCB28      LD B,SRA (IX+d)*
>DDCB29      LD C,SRA (IX+d)*
>DDCB2A      LD D,SRA (IX+d)*
>DDCB2B      LD E,SRA (IX+d)*
>DDCB2C      LD H,SRA (IX+d)*
>DDCB2D      LD L,SRA (IX+d)*
>DDCB2E      SRA (IX+d)
>DDCB2F      LD A,SRA (IX+d)*
>DDCB30      LD B,SLL (IX+d)*
>DDCB31      LD C,SLL (IX+d)*
>DDCB32      LD D,SLL (IX+d)*
>DDCB33      LD E,SLL (IX+d)*
>DDCB34      LD H,SLL (IX+d)*
>DDCB35      LD L,SLL (IX+d)*
>DDCB36      SLL (IX+d)*
>DDCB37      LD A,SLL (IX+d)*
>DDCB38      LD B,SRL (IX+d)*
>DDCB39      LD C,SRL (IX+d)*
>DDCB3A      LD D,SRL (IX+d)*
>DDCB3B      LD E,SRL (IX+d)*
>DDCB3C      LD H,SRL (IX+d)*
>DDCB3D      LD L,SRL (IX+d)*
>DDCB3E      SRL (IX+d)
>DDCB3F      LD A,SRL (IX+d)*
>DDCB40      BIT 0,(IX+d)*
>DDCB41      BIT 0,(IX+d)*
>DDCB42      BIT 0,(IX+d)*
>DDCB43      BIT 0,(IX+d)*
>DDCB44      BIT 0,(IX+d)*
>DDCB45      BIT 0,(IX+d)*
>DDCB46      BIT 0,(IX+d)
>DDCB47      BIT 0,(IX+d)*
>DDCB48      BIT 1,(IX+d)*
>DDCB49      BIT 1,(IX+d)*
>DDCB4A      BIT 1,(IX+d)*
>DDCB4B      BIT 1,(IX+d)*
>DDCB4C      BIT 1,(IX+d)*
>DDCB4D      BIT 1,(IX+d)*
>DDCB4E      BIT 1,(IX+d)
>DDCB4F      BIT 1,(IX+d)*
>DDCB50      BIT 2,(IX+d)*
>DDCB51      BIT 2,(IX+d)*
>DDCB52      BIT 2,(IX+d)*
>DDCB53      BIT 2,(IX+d)*
>DDCB54      BIT 2,(IX+d)*
>DDCB55      BIT 2,(IX+d)*
>DDCB56      BIT 2,(IX+d)
>DDCB57      BIT 2,(IX+d)*
>DDCB58      BIT 3,(IX+d)*
>DDCB59      BIT 3,(IX+d)*
>DDCB5A      BIT 3,(IX+d)*
>DDCB5B      BIT 3,(IX+d)*
>DDCB5C      BIT 3,(IX+d)*
>DDCB5D      BIT 3,(IX+d)*
>DDCB5E      BIT 3,(IX+d)
>DDCB5F      BIT 3,(IX+d)*
>DDCB60      BIT 4,(IX+d)*
>DDCB61      BIT 4,(IX+d)*
>DDCB62      BIT 4,(IX+d)*
>DDCB63      BIT 4,(IX+d)*
>DDCB64      BIT 4,(IX+d)*
>DDCB65      BIT 4,(IX+d)*
>DDCB66      BIT 4,(IX+d)
>DDCB67      BIT 4,(IX+d)*
>DDCB68      BIT 5,(IX+d)*
>DDCB69      BIT 5,(IX+d)*
>DDCB6A      BIT 5,(IX+d)*
>DDCB6B      BIT 5,(IX+d)*
>DDCB6C      BIT 5,(IX+d)*
>DDCB6D      BIT 5,(IX+d)*
>DDCB6E      BIT 5,(IX+d)
>DDCB6F      BIT 5,(IX+d)*
>DDCB70      BIT 6,(IX+d)*
>DDCB71      BIT 6,(IX+d)*
>DDCB72      BIT 6,(IX+d)*
>DDCB73      BIT 6,(IX+d)*
>DDCB74      BIT 6,(IX+d)*
>DDCB75      BIT 6,(IX+d)*
>DDCB76      BIT 6,(IX+d)
>DDCB77      BIT 6,(IX+d)*
>DDCB78      BIT 7,(IX+d)*
>DDCB79      BIT 7,(IX+d)*
>DDCB7A      BIT 7,(IX+d)*
>DDCB7B      BIT 7,(IX+d)*
>DDCB7C      BIT 7,(IX+d)*
>DDCB7D      BIT 7,(IX+d)*
>DDCB7E      BIT 7,(IX+d)
>DDCB7F      BIT 7,(IX+d)*
>DDCB80      LD B,RES 0,(IX+d)*
>DDCB81      LD C,RES 0,(IX+d)*
>DDCB82      LD D,RES 0,(IX+d)*
>DDCB83      LD E,RES 0,(IX+d)*
>DDCB84      LD H,RES 0,(IX+d)*
>DDCB85      LD L,RES 0,(IX+d)*
>DDCB86      RES 0,(IX+d)
>DDCB87      LD A,RES 0,(IX+d)*
>DDCB88      LD B,RES 1,(IX+d)*
>DDCB89      LD C,RES 1,(IX+d)*
>DDCB8A      LD D,RES 1,(IX+d)*
>DDCB8B      LD E,RES 1,(IX+d)*
>DDCB8C      LD H,RES 1,(IX+d)*
>DDCB8D      LD L,RES 1,(IX+d)*
>DDCB8E      RES 1,(IX+d)
>DDCB8F      LD A,RES 1,(IX+d)*
>DDCB90      LD B,RES 2,(IX+d)*
>DDCB91      LD C,RES 2,(IX+d)*
>DDCB92      LD D,RES 2,(IX+d)*
>DDCB93      LD E,RES 2,(IX+d)*
>DDCB94      LD H,RES 2,(IX+d)*
>DDCB95      LD L,RES 2,(IX+d)*
>DDCB96      RES 2,(IX+d)
>DDCB97      LD A,RES 2,(IX+d)*
>DDCB98      LD B,RES 3,(IX+d)*
>DDCB99      LD C,RES 3,(IX+d)*
>DDCB9A      LD D,RES 3,(IX+d)*
>DDCB9B      LD E,RES 3,(IX+d)*
>DDCB9C      LD H,RES 3,(IX+d)*
>DDCB9D      LD L,RES 3,(IX+d)*
>DDCB9E      RES 3,(IX+d)
>DDCB9F      LD A,RES 3,(IX+d)*
>DDCBA0      LD B,RES 4,(IX+d)*
>DDCBA1      LD C,RES 4,(IX+d)*
>DDCBA2      LD D,RES 4,(IX+d)*
>DDCBA3      LD E,RES 4,(IX+d)*
>DDCBA4      LD H,RES 4,(IX+d)*
>DDCBA5      LD L,RES 4,(IX+d)*
>DDCBA6      RES 4,(IX+d)
>DDCBA7      LD A,RES 4,(IX+d)*
>DDCBA8      LD B,RES 5,(IX+d)*
>DDCBA9      LD C,RES 5,(IX+d)*
>DDCBAA      LD D,RES 5,(IX+d)*
>DDCBAB      LD E,RES 5,(IX+d)*
>DDCBAC      LD H,RES 5,(IX+d)*
>DDCBAD      LD L,RES 5,(IX+d)*
>DDCBAE      RES 5,(IX+d)
>DDCBAF      LD A,RES 5,(IX+d)*
>DDCBB0      LD B,RES 6,(IX+d)*
>DDCBB1      LD C,RES 6,(IX+d)*
>DDCBB2      LD D,RES 6,(IX+d)*
>DDCBB3      LD E,RES 6,(IX+d)*
>DDCBB4      LD H,RES 6,(IX+d)*
>DDCBB5      LD L,RES 6,(IX+d)*
>DDCBB6      RES 6,(IX+d)
>DDCBB7      LD A,RES 6,(IX+d)*
>DDCBB8      LD B,RES 7,(IX+d)*
>DDCBB9      LD C,RES 7,(IX+d)*
>DDCBBA      LD D,RES 7,(IX+d)*
>DDCBBB      LD E,RES 7,(IX+d)*
>DDCBBC      LD H,RES 7,(IX+d)*
>DDCBBD      LD L,RES 7,(IX+d)*
>DDCBBE      RES 7,(IX+d)
>DDCBBF      LD A,RES 7,(IX+d)*
>DDCBC0      LD B,SET 0,(IX+d)*
>DDCBC1      LD C,SET 0,(IX+d)*
>DDCBC2      LD D,SET 0,(IX+d)*
>DDCBC3      LD E,SET 0,(IX+d)*
>DDCBC4      LD H,SET 0,(IX+d)*
>DDCBC5      LD L,SET 0,(IX+d)*
>DDCBC6      SET 0,(IX+d)
>DDCBC7      LD A,SET 0,(IX+d)*
>DDCBC8      LD B,SET 1,(IX+d)*
>DDCBC9      LD C,SET 1,(IX+d)*
>DDCBCA      LD D,SET 1,(IX+d)*
>DDCBCB      LD E,SET 1,(IX+d)*
>DDCBCC      LD H,SET 1,(IX+d)*
>DDCBCD      LD L,SET 1,(IX+d)*
>DDCBCE      SET 1,(IX+d)
>DDCBCF      LD A,SET 1,(IX+d)*
>DDCBD0      LD B,SET 2,(IX+d)*
>DDCBD1      LD C,SET 2,(IX+d)*
>DDCBD2      LD D,SET 2,(IX+d)*
>DDCBD3      LD E,SET 2,(IX+d)*
>DDCBD4      LD H,SET 2,(IX+d)*
>DDCBD5      LD L,SET 2,(IX+d)*
>DDCBD6      SET 2,(IX+d)
>DDCBD7      LD A,SET 2,(IX+d)*
>DDCBD8      LD B,SET 3,(IX+d)*
>DDCBD9      LD C,SET 3,(IX+d)*
>DDCBDA      LD D,SET 3,(IX+d)*
>DDCBDB      LD E,SET 3,(IX+d)*
>DDCBDC      LD H,SET 3,(IX+d)*
>DDCBDD      LD L,SET 3,(IX+d)*
>DDCBDE      SET 3,(IX+d)
>DDCBDF      LD A,SET 3,(IX+d)*
>DDCBE0      LD B,SET 4,(IX+d)*
>DDCBE1      LD C,SET 4,(IX+d)*
>DDCBE2      LD D,SET 4,(IX+d)*
>DDCBE3      LD E,SET 4,(IX+d)*
>DDCBE4      LD H,SET 4,(IX+d)*
>DDCBE5      LD L,SET 4,(IX+d)*
>DDCBE6      SET 4,(IX+d)
>DDCBE7      LD A,SET 4,(IX+d)*
>DDCBE8      LD B,SET 5,(IX+d)*
>DDCBE9      LD C,SET 5,(IX+d)*
>DDCBEA      LD D,SET 5,(IX+d)*
>DDCBEB      LD E,SET 5,(IX+d)*
>DDCBEC      LD H,SET 5,(IX+d)*
>DDCBED      LD L,SET 5,(IX+d)*
>DDCBEE      SET 5,(IX+d)
>DDCBEF      LD A,SET 5,(IX+d)*
>DDCBF0      LD B,SET 6,(IX+d)*
>DDCBF1      LD C,SET 6,(IX+d)*
>DDCBF2      LD D,SET 6,(IX+d)*
>DDCBF3      LD E,SET 6,(IX+d)*
>DDCBF4      LD H,SET 6,(IX+d)*
>DDCBF5      LD L,SET 6,(IX+d)*
>DDCBF6      SET 6,(IX+d)
>DDCBF7      LD A,SET 6,(IX+d)*
>DDCBF8      LD B,SET 7,(IX+d)*
>DDCBF9      LD C,SET 7,(IX+d)*
>DDCBFA      LD D,SET 7,(IX+d)*
>DDCBB       LD E,SET 7,(IX+d)*
>DDCBFC      LD H,SET 7,(IX+d)*
>DDCBFD      LD L,SET 7,(IX+d)*
>DDCBFE      SET 7,(IX+d)
>DDCBFF      LD A,SET 7,(IX+d)*
>DDE1        POP IX
>DDE3        EX (SP),IX
>DDE5        PUSH IX
>DDE9        JP (IX)
>DDF9        LD SP,IX
>DE          SBC A,n
>DF          RST 18H
>E0          RET PO
>E1          POP HL
>E2          JP PO,nn
>E3          EX (SP),HL
>E4          CALL PO,nn
>E5          PUSH HL
>E6          AND n
>E7          RST 20H
>E8          RET PE
>E9          JP (HL)
>EA          JP PE,nn
>EB          EX DE,HL
>EC          CALL PE,nn
>ED40        IN B,(C)
>ED41        OUT (C),B
>ED42        SBC HL,BC
>ED43        LD (nn),BC
>ED44        NEG
>ED45        RETN
>ED46        IM 0
>ED47        LD I,A
>ED48        IN C,(C)
>ED49        OUT (C),C
>ED4A        ADC HL,BC
>ED4B        LD BC,(nn)
>ED4C        NEG*
>ED4D        RETI
>ED4E        IM 0/1*
>ED4F        LD R,A
>ED50        IN D,(C)
>ED51        OUT (C),D
>ED52        SBC HL,DE
>ED53        LD (nn),DE
>ED54        NEG*
>ED55        RETN*
>ED56        IM 1
>ED57        LD A,I
>ED58        IN E,(C)
>ED59        OUT (C),E
>ED5A        ADC HL,DE
>ED5B        LD DE,(nn)
>ED5C        NEG*
>ED5D        RETN*
>ED5E        IM 2
>ED5F        LD A,R
>ED60        IN H,(C)
>ED61        OUT (C),H
>ED62        SBC HL,HL
>ED63        LD (nn),HL
>ED64        NEG*
>ED65        RETN*
>ED66        IM 0*
>ED67        RRD
>ED68        IN L,(C)
>ED69        OUT (C),L
>ED6A        ADC HL,HL
>ED6B        LD HL,(nn)
>ED6C        NEG*
>ED6D        RETN*
>ED6E        IM 0/1*
>ED6F        RLD
>ED70        IN F,(C)* / IN (C)*
>ED71        OUT (C),0*
>ED72        SBC HL,SP
>ED73        LD (nn),SP
>ED74        NEG*
>ED75        RETN*
>ED76        IM 1*
>ED78        IN A,(C)
>ED79        OUT (C),A
>ED7A        ADC HL,SP
>ED7B        LD SP,(nn)
>ED7C        NEG*
>ED7D        RETN*
>ED7E        IM 2*
>EDA0        LDI
>EDA1        CPI
>EDA2        INI
>EDA3        OUTI
>EDA8        LDD
>EDA9        CPD
>EDAA        IND
>EDAB        OUTD
>EDB0        LDIR
>EDB1        CPIR
>EDB2        INIR
>EDB3        OTIR
>EDB8        LDDR
>EDB9        CPDR
>EDBA        INDR
>EDBB        OTDR
>EE          XOR n
>EF          RST 28H
>F0          RET P
>F1          POP AF
>F2          JP P,nn
>F3          DI
>F4          CALL P,nn
>F5          PUSH AF
>F6          OR n
>F7          RST 30H
>F8          RET M
>F9          LD SP,HL
>FA          JP M,nn
>FB          EI
>FC          CALL M,nn
>FD09        ADD IY,BC
>FD19        ADD IY,DE
>FD21        LD IY,nn
>FD22        LD (nn),IY
>FD23        INC IY
>FD24        INC IYH*
>FD25        DEC IYH*
>FD26        LD IYH,n*
>FD29        ADD IY,IY
>FD2A        LD IY,(nn)
>FD2B        DEC IY
>FD2C        INC IYL*
>FD2D        DEC IYL*
>FD2E        LD IYL,n*
>FD34        INC (IY+d)
>FD35        DEC (IY+d)
>FD36        LD (IY+d),n
>FD39        ADD IY,SP
>FD44        LD B,IYH*
>FD45        LD B,IYL*
>FD46        LD B,(IY+d)
>FD4C        LD C,IYH*
>FD4D        LD C,IYL*
>FD4E        LD C,(IY+d)
>FD54        LD D,IYH*
>FD55        LD D,IYL*
>FD56        LD D,(IY+d)
>FD5C        LD E,IYH*
>FD5D        LD E,IYL*
>FD5E        LD E,(IY+d)
>FD60        LD IYH,B*
>FD61        LD IYH,C*
>FD62        LD IYH,D*
>FD63        LD IYH,E*
>FD64        LD IYH,IYH*
>FD65        LD IYH,IYL*
>FD66        LD H,(IY+d)
>FD67        LD IYH,A*
>FD68        LD IYL,B*
>FD69        LD IYL,C*
>FD6A        LD IYL,D*
>FD6B        LD IYL,E*
>FD6C        LD IYL,IYH*
>FD6D        LD IYL,IYL*
>FD6E        LD L,(IY+d)
>FD6F        LD IYL,A*
>FD70        LD (IY+d),B
>FD71        LD (IY+d),C
>FD72        LD (IY+d),D
>FD73        LD (IY+d),E
>FD74        LD (IY+d),H
>FD75        LD (IY+d),L
>FD77        LD (IY+d),A
>FD7C        LD A,IYH*
>FD7D        LD A,IYL*
>FD7E        LD A,(IY+d)
>FD84        ADD A,IYH*
>FD85        ADD A,IYL*
>FD86        ADD A,(IY+d)
>FD8C        ADC A,IYH*
>FD8D        ADC A,IYL*
>FD8E        ADC A,(IY+d)
>FD94        SUB IYH*
>FD95        SUB IYL*
>FD96        SUB (IY+d)
>FD9C        SBC A,IYH*
>FD9D        SBC A,IYL*
>FD9E        SBC A,(IY+d)
>FDA4        AND IYH*
>FDA5        AND IYL*
>FDA6        AND (IY+d)
>FDAC        XOR IYH*
>FDAD        XOR IYL*
>FDAE        XOR (IY+d)
>FDB4        OR IYH*
>FDB5        OR IYL*
>FDB6        OR (IY+d)
>FDBC        CP IYH*
>FDBD        CP IYL*
>FDBE        CP (IY+d)
>FDCB00      LD B,RLC (IY+d)*
>FDCB01      LD C,RLC (IY+d)*
>FDCB02      LD D,RLC (IY+d)*
>FDCB03      LD E,RLC (IY+d)*
>FDCB04      LD H,RLC (IY+d)*
>FDCB05      LD L,RLC (IY+d)*
>FDCB06      RLC (IY+d)
>FDCB07      LD A,RLC (IY+d)*
>FDCB08      LD B,RRC (IY+d)*
>FDCB09      LD C,RRC (IY+d)*
>FDCB0A      LD D,RRC (IY+d)*
>FDCB0B      LD E,RRC (IY+d)*
>FDCB0C      LD H,RRC (IY+d)*
>FDCB0D      LD L,RRC (IY+d)*
>FDCB0E      RRC (IY+d)
>FDCB0F      LD A,RRC (IY+d)*
>FDCB10      LD B,RL (IY+d)*
>FDCB11      LD C,RL (IY+d)*
>FDCB12      LD D,RL (IY+d)*
>FDCB13      LD E,RL (IY+d)*
>FDCB14      LD H,RL (IY+d)*
>FDCB15      LD L,RL (IY+d)*
>FDCB16      RL (IY+d)
>FDCB17      LD A,RL (IY+d)*
>FDCB18      LD B,RR (IY+d)*
>FDCB19      LD C,RR (IY+d)*
>FDCB1A      LD D,RR (IY+d)*
>FDCB1B      LD E,RR (IY+d)*
>FDCB1C      LD H,RR (IY+d)*
>FDCB1D      LD L,RR (IY+d)*
>FDCB1E      RR (IY+d)
>FDCB1F      LD A,RR (IY+d)*
>FDCB20      LD B,SLA (IY+d)*
>FDCB21      LD C,SLA (IY+d)*
>FDCB22      LD D,SLA (IY+d)*
>FDCB23      LD E,SLA (IY+d)*
>FDCB24      LD H,SLA (IY+d)*
>FDCB25      LD L,SLA (IY+d)*
>FDCB26      SLA (IY+d)
>FDCB27      LD A,SLA (IY+d)*
>FDCB28      LD B,SRA (IY+d)*
>FDCB29      LD C,SRA (IY+d)*
>FDCB2A      LD D,SRA (IY+d)*
>FDCB2B      LD E,SRA (IY+d)*
>FDCB2C      LD H,SRA (IY+d)*
>FDCB2D      LD L,SRA (IY+d)*
>FDCB2E      SRA (IY+d)
>FDCB2F      LD A,SRA (IY+d)*
>FDCB30      LD B,SLL (IY+d)*
>FDCB31      LD C,SLL (IY+d)*
>FDCB32      LD D,SLL (IY+d)*
>FDCB33      LD E,SLL (IY+d)*
>FDCB34      LD H,SLL (IY+d)*
>FDCB35      LD L,SLL (IY+d)*
>FDCB36      SLL (IY+d)*
>FDCB37      LD A,SLL (IY+d)*
>FDCB38      LD B,SRL (IY+d)*
>FDCB39      LD C,SRL (IY+d)*
>FDCB3A      LD D,SRL (IY+d)*
>FDCB3B      LD E,SRL (IY+d)*
>FDCB3C      LD H,SRL (IY+d)*
>FDCB3D      LD L,SRL (IY+d)*
>FDCB3E      SRL (IY+d)
>FDCB3F      LD A,SRL (IY+d)*
>FDCB40      BIT 0,(IY+d)*
>FDCB41      BIT 0,(IY+d)*
>FDCB42      BIT 0,(IY+d)*
>FDCB43      BIT 0,(IY+d)*
>FDCB44      BIT 0,(IY+d)*
>FDCB45      BIT 0,(IY+d)*
>FDCB46      BIT 0,(IY+d)
>FDCB47      BIT 0,(IY+d)*
>FDCB48      BIT 1,(IY+d)*
>FDCB49      BIT 1,(IY+d)*
>FDCB4A      BIT 1,(IY+d)*
>FDCB4B      BIT 1,(IY+d)*
>FDCB4C      BIT 1,(IY+d)*
>FDCB4D      BIT 1,(IY+d)*
>FDCB4E      BIT 1,(IY+d)
>FDCB4F      BIT 1,(IY+d)*
>FDCB50      BIT 2,(IY+d)*
>FDCB51      BIT 2,(IY+d)*
>FDCB52      BIT 2,(IY+d)*
>FDCB53      BIT 2,(IY+d)*
>FDCB54      BIT 2,(IY+d)*
>FDCB55      BIT 2,(IY+d)*
>FDCB56      BIT 2,(IY+d)
>FDCB57      BIT 2,(IY+d)*
>FDCB58      BIT 3,(IY+d)*
>FDCB59      BIT 3,(IY+d)*
>FDCB5A      BIT 3,(IY+d)*
>FDCB5B      BIT 3,(IY+d)*
>FDCB5C      BIT 3,(IY+d)*
>FDCB5D      BIT 3,(IY+d)*
>FDCB5E      BIT 3,(IY+d)
>FDCB5F      BIT 3,(IY+d)*
>FDCB60      BIT 4,(IY+d)*
>FDCB61      BIT 4,(IY+d)*
>FDCB62      BIT 4,(IY+d)*
>FDCB63      BIT 4,(IY+d)*
>FDCB64      BIT 4,(IY+d)*
>FDCB65      BIT 4,(IY+d)*
>FDCB66      BIT 4,(IY+d)
>FDCB67      BIT 4,(IY+d)*
>FDCB68      BIT 5,(IY+d)*
>FDCB69      BIT 5,(IY+d)*
>FDCB6A      BIT 5,(IY+d)*
>FDCB6B      BIT 5,(IY+d)*
>FDCB6C      BIT 5,(IY+d)*
>FDCB6D      BIT 5,(IY+d)*
>FDCB6E      BIT 5,(IY+d)
>FDCB6F      BIT 5,(IY+d)*
>FDCB70      BIT 6,(IY+d)*
>FDCB71      BIT 6,(IY+d)*
>FDCB72      BIT 6,(IY+d)*
>FDCB73      BIT 6,(IY+d)*
>FDCB74      BIT 6,(IY+d)*
>FDCB75      BIT 6,(IY+d)*
>FDCB76      BIT 6,(IY+d)
>FDCB77      BIT 6,(IY+d)*
>FDCB78      BIT 7,(IY+d)*
>FDCB79      BIT 7,(IY+d)*
>FDCB7A      BIT 7,(IY+d)*
>FDCB7B      BIT 7,(IY+d)*
>FDCB7C      BIT 7,(IY+d)*
>FDCB7D      BIT 7,(IY+d)*
>FDCB7E      BIT 7,(IY+d)
>FDCB7F      BIT 7,(IY+d)*
>FDCB80      LD B,RES 0,(IY+d)*
>FDCB81      LD C,RES 0,(IY+d)*
>FDCB82      LD D,RES 0,(IY+d)*
>FDCB83      LD E,RES 0,(IY+d)*
>FDCB84      LD H,RES 0,(IY+d)*
>FDCB85      LD L,RES 0,(IY+d)*
>FDCB86      RES 0,(IY+d)
>FDCB87      LD A,RES 0,(IY+d)*
>FDCB88      LD B,RES 1,(IY+d)*
>FDCB89      LD C,RES 1,(IY+d)*
>FDCB8A      LD D,RES 1,(IY+d)*
>FDCB8B      LD E,RES 1,(IY+d)*
>FDCB8C      LD H,RES 1,(IY+d)*
>FDCB8D      LD L,RES 1,(IY+d)*
>FDCB8E      RES 1,(IY+d)
>FDCB8F      LD A,RES 1,(IY+d)*
>FDCB90      LD B,RES 2,(IY+d)*
>FDCB91      LD C,RES 2,(IY+d)*
>FDCB92      LD D,RES 2,(IY+d)*
>FDCB93      LD E,RES 2,(IY+d)*
>FDCB94      LD H,RES 2,(IY+d)*
>FDCB95      LD L,RES 2,(IY+d)*
>FDCB96      RES 2,(IY+d)
>FDCB97      LD A,RES 2,(IY+d)*
>FDCB98      LD B,RES 3,(IY+d)*
>FDCB99      LD C,RES 3,(IY+d)*
>FDCB9A      LD D,RES 3,(IY+d)*
>FDCB9B      LD E,RES 3,(IY+d)*
>FDCB9C      LD H,RES 3,(IY+d)*
>FDCB9D      LD L,RES 3,(IY+d)*
>FDCB9E      RES 3,(IY+d)
>FDCB9F      LD A,RES 3,(IY+d)*
>FDCBA0      LD B,RES 4,(IY+d)*
>FDCBA1      LD C,RES 4,(IY+d)*
>FDCBA2      LD D,RES 4,(IY+d)*
>FDCBA3      LD E,RES 4,(IY+d)*
>FDCBA4      LD H,RES 4,(IY+d)*
>FDCBA5      LD L,RES 4,(IY+d)*
>FDCBA6      RES 4,(IY+d)
>FDCBA7      LD A,RES 4,(IY+d)*
>FDCBA8      LD B,RES 5,(IY+d)*
>FDCBA9      LD C,RES 5,(IY+d)*
>FDCBAA      LD D,RES 5,(IY+d)*
>FDCBAB      LD E,RES 5,(IY+d)*
>FDCBAC      LD H,RES 5,(IY+d)*
>FDCBAD      LD L,RES 5,(IY+d)*
>FDCBAE      RES 5,(IY+d)
>FDCBAF      LD A,RES 5,(IY+d)*
>FDCBB0      LD B,RES 6,(IY+d)*
>FDCBB1      LD C,RES 6,(IY+d)*
>FDCBB2      LD D,RES 6,(IY+d)*
>FDCBB3      LD E,RES 6,(IY+d)*
>FDCBB4      LD H,RES 6,(IY+d)*
>FDCBB5      LD L,RES 6,(IY+d)*
>FDCBB6      RES 6,(IY+d)
>FDCBB7      LD A,RES 6,(IY+d)*
>FDCBB8      LD B,RES 7,(IY+d)*
>FDCBB9      LD C,RES 7,(IY+d)*
>FDCBBA      LD D,RES 7,(IY+d)*
>FDCBBB      LD E,RES 7,(IY+d)*
>FDCBBC      LD H,RES 7,(IY+d)*
>FDCBBD      LD L,RES 7,(IY+d)*
>FDCBBE      RES 7,(IY+d)
>FDCBBF      LD A,RES 7,(IY+d)*
>FDCBC0      LD B,SET 0,(IY+d)*
>FDCBC1      LD C,SET 0,(IY+d)*
>FDCBC2      LD D,SET 0,(IY+d)*
>FDCBC3      LD E,SET 0,(IY+d)*
>FDCBC4      LD H,SET 0,(IY+d)*
>FDCBC5      LD L,SET 0,(IY+d)*
>FDCBC6      SET 0,(IY+d)
>FDCBC7      LD A,SET 0,(IY+d)*
>FDCBC8      LD B,SET 1,(IY+d)*
>FDCBC9      LD C,SET 1,(IY+d)*
>FDCBCA      LD D,SET 1,(IY+d)*
>FDCBCB      LD E,SET 1,(IY+d)*
>FDCBCC      LD H,SET 1,(IY+d)*
>FDCBCD      LD L,SET 1,(IY+d)*
>FDCBCE      SET 1,(IY+d)
>FDCBCF      LD A,SET 1,(IY+d)*
>FDCBD0      LD B,SET 2,(IY+d)*
>FDCBD1      LD C,SET 2,(IY+d)*
>FDCBD2      LD D,SET 2,(IY+d)*
>FDCBD3      LD E,SET 2,(IY+d)*
>FDCBD4      LD H,SET 2,(IY+d)*
>FDCBD5      LD L,SET 2,(IY+d)*
>FDCBD6      SET 2,(IY+d)
>FDCBD7      LD A,SET 2,(IY+d)*
>FDCBD8      LD B,SET 3,(IY+d)*
>FDCBD9      LD C,SET 3,(IY+d)*
>FDCBDA      LD D,SET 3,(IY+d)*
>FDCBDB      LD E,SET 3,(IY+d)*
>FDCBDC      LD H,SET 3,(IY+d)*
>FDCBDD      LD L,SET 3,(IY+d)*
>FDCBDE      SET 3,(IY+d)
>FDCBDF      LD A,SET 3,(IY+d)*
>FDCBE0      LD B,SET 4,(IY+d)*
>FDCBE1      LD C,SET 4,(IY+d)*
>FDCBE2      LD D,SET 4,(IY+d)*
>FDCBE3      LD E,SET 4,(IY+d)*
>FDCBE4      LD H,SET 4,(IY+d)*
>FDCBE5      LD L,SET 4,(IY+d)*
>FDCBE6      SET 4,(IY+d)
>FDCBE7      LD A,SET 4,(IY+d)*
>FDCBE8      LD B,SET 5,(IY+d)*
>FDCBE9      LD C,SET 5,(IY+d)*
>FDCBEA      LD D,SET 5,(IY+d)*
>FDCBEB      LD E,SET 5,(IY+d)*
>FDCBEC      LD H,SET 5,(IY+d)*
>FDCBED      LD L,SET 5,(IY+d)*
>FDCBEE      SET 5,(IY+d)
>FDCBEF      LD A,SET 5,(IY+d)*
>FDCBF0      LD B,SET 6,(IY+d)*
>FDCBF1      LD C,SET 6,(IY+d)*
>FDCBF2      LD D,SET 6,(IY+d)*
>FDCBF3      LD E,SET 6,(IY+d)*
>FDCBF4      LD H,SET 6,(IY+d)*
>FDCBF5      LD L,SET 6,(IY+d)*
>FDCBF6      SET 6,(IY+d)
>FDCBF7      LD A,SET 6,(IY+d)*
>FDCBF8      LD B,SET 7,(IY+d)*
>FDCBF9      LD C,SET 7,(IY+d)*
>FDCBFA      LD D,SET 7,(IY+d)*
>FDCBFB      LD E,SET 7,(IY+d)*
>FDCBFC      LD H,SET 7,(IY+d)*
>FDCBFD      LD L,SET 7,(IY+d)*
>FDCBFE      SET 7,(IY+d)
>FDCBFF      LD A,SET 7,(IY+d)*
>FDE1        POP IY
>FDE3        EX (SP),IY
>FDE5        PUSH IY
>FDE9        JP (IY)
>FDF9        LD SP,IY
>FE          CP n
>FF          RST 38H
>end of file