program MyProgram;
var  
   index: byte; 
	bgcol,k3, x,y,time,time2,idx,i,j,road, k,ms_shift,k2,current, ffld,val,a,b, cur_col, cur_start,l,m,dy,scroll,dscroll: byte = 0;
	sx,dsx,tt,speed: byte =1;
	cc, i_, k_, k2_, j_:byte = 0;
	shifts : array[16] of byte;
	shifts2 : array[16] of byte;
	int : integer;

	colorsRedhues : array [16] of byte = (  0,11,0,0  );
	
	roads: array[32] of byte = (
	%11110000,	%00000000,
	%11100000,	%00000001,
	%11000000,	%00000011,
	%10000000,	%00000111,
	%00000000,	%00001111,
	%00000000,	%00011110,
	%00000000,	%00111100,
	%00000000,	%01111000,
	%00000000,	%11110000,
	%00000001,	%11100000,
	%00000011,	%11000000,
	%00000111,	%10000000,
	%00001111,	%00000000,
	%00011100,	%00000000,
	%00111000,	%00000000,
	%01110000,	%00000000,




	);
//	textcols : array[7] of byte = (7,4,4,3,3,11, 11);



@define roadBlock $3D

	charset:incbin("charsets/charset.bin", $2000);
	sprites : incbin("images/trse.bin",$2800);

	sine2:array[256] of byte;
	tab:array[256] of byte;


//@define debugRaster 1
	


	waves : string=(   
//					"          ",255,
					"LEMONSPAWN  ",255,
					  "PRESENTS    ",255,
					  "$4K         ",255,
					  "DREAMS     ",255,
					  "CODE        ",255,
					  "LEUAT        ",255,
					  "MUSIC        ",255,
					  "WARLORD      ",255,
					  "DEVELOPED      ",255,
					  "WITH        ",255,
					  "TRSE        ",255,
					0); 


	@define starPos $b0
	@define starPosEnd $b8
	@define starsY 7
	@define starsPerLine 2
	@define starsLines 5

	star_x:array[24] of byte;	
	star_dx:array[24] of byte;	
	star_ddx:array[24] of byte;	

@define FontTabPos $2A00

	zp,p1,p2,tp,tp2:pointer;

	// Used in main
	p3,p4,zp2 : pointer;

	uct: incsid("music/exhale2B.sid",2);
	
//	cs: incbin("charsets/waves.bin",$2800);


	fadeBlue : array [16] of byte = (11,6,6,12,4,14,15,1,1,15,14,4,12,6,6,11); 



	text : string = ("         LEMONSPAWN PRESENTS      $4K DREAMS       A SMALL CRACKTRO          PARTICIPATING IN THE 2018 CSDB INTRO CREATION COMPETITION                ",
					" CODE LEUAT      MUSIC WARLORD       THANKS TO EVERYONE WHO ARE SUPPORTING THE CONTINUOUS DEVELOPMENT OF TRSE                 ");

	fontTable : array[16] of byte = ($20, $7e, $7C, $E2, 
									$6C, $7f, $E1,  $Fb,
									$7b, $61, $ff, $ec,
									$62, $fc, $fe, $53);



@startblock @FontTabPos FontTab
	FontTab : array[256] of byte;
@endblock

	
@include "packed_resources1.ras"

@define useKernal 0
@define ypos 16

interrupt RasterBar();
interrupt RasterLower();

procedure MoveRestSprites();
procedure UpdateRoad();
procedure PrintWave();


//procedure PrintNumberOfWaves();

@define rypos 14

procedure SetupScroll();
begin
	k2:=0-time;
	for k:=0 to 4 do begin
		ms_shift:=sine[time+k2];// -sine[time*2+k2*2+3]/4;
		if (dscroll<>0) then begin
			shifts[k]:=(7-ms_shift)&7;
		end;
//		ms_shift:=ms_shift/8;
		shifts2[k]:=(ms_shift>>3);	
//		if (dscroll<>0) then
		if (k=1) then shifts[k]:=7-dscroll;
		k2:=k2+44;
	end;
end;


procedure PrintWaves();
begin
	moveto(0,@ypos-2,$04);

	p1:=screenmemory;
	p1:=p1+40;
	
	a:=0;
	b:=40;
	i:=sine[time];
	shifts2[0]:=i/8;
	shifts[0]:=7-i&7;
	ms_shift:=shifts2[0];
	PrintWave();
	moveto(0,@ypos+4,$04);

	p1:=screenmemory;
	p1:=p1+40;
	
	i:=sine[time+64];
	shifts2[2]:=i/8;
	shifts[2]:=7-i&7;
	ms_shift:=shifts2[2];
	
	PrintWave();


end;

@define cwait 128

procedure RenderCredzChar();
begin
	k:=tp[0];

	if (k=0) then begin
		tp:=#text;
		scroll:=0;
		return();

	end;


	if (k=@cwait) then begin
		dy:=tp[1];
		tp:=tp+2;
		return();

	end;

		k:=k*2;
		asm("
			ldy k
			lda @FontTabPos,y
			sta zp
			iny
			lda @FontTabPos,y
			sta zp+1

		");


	screenmemory:=$0400+@ypos*40+39;
	idx:=1;
	l:=scroll*2;
	m:=scroll*2+2;
	for y:=0 to 8 step 2 do begin
		for x:=l to m step 2 do begin
			
			k:=getbit(zp[y],7-x);
			k:=k+getbit(zp[y],6-x)*2;
			k:=k+getbit(zp[y+1],6-x)*4;
			k:=k+getbit(zp[y+1],7-x)*8;


			k:=k&15;
			if (tp[0]=$20) then k:=0;
			screenmemory[0]:=fontTable[k];
//			h2[x/2]:=cx;
		end;
		screenmemory:=screenmemory+40;
	end;
	inc(scroll);
	if (scroll=4) then begin
		tp:=tp+1;
		scroll:=0;
	end;

	dy:=0;
//	SCREEN_BG_COLOR:=BLACK;
end;


procedure SetupFontTab();
begin
	p1:=@FontTabPos;
	for i:=0 to 128 do begin	
		k:=i;
		if (k>=64) then
			k:=k-64;

		zp:=$2000;

		if k>=31 then begin
			k:=k-31;
			zp:=zp+(31*8);
		end;
		if (k<>0) then 
			zp:=zp +k*8;

		k:=i*2;
		asm("
			ldy k
			lda zp
			sta (p1),y
			lda zp+1
			iny
			sta (p1),y

		");
//		inczp(p1,2);

	end;

end;




procedure SetupCopyText();
begin
	p3:=$2000+128*8;
	p4:=$2000+128*8+16*8;
//	tt:=time2;
//	c:=0;
	time2:=time2+1;
	sx:=0-sine[time2+32]/12+4;
//	if (time&7=3) then 
//		dec(sx);

	if (time2>=253) then begin
		while (tp2[0]<>255) do
			tp2:=tp2+1;
			
		tp2:=tp2+1;
		if (tp2[0]=0) then tp2:=#waves;			
		time2:=0;
//		sx:=12;
	end;

	cc:=0;
	tt:=time2*4;
//	if (a<>0) then begin inczp(p3,a*8);inczp(p4,a*8);end;


end;


procedure CopyText();
begin
	for i_:=a to b  do begin
		k_:=tp2[i_]*2;
//		if (tp2[i_]=255) then k_:=$40;
		asm("
			
			ldy k_
			lda @FontTabPos,y
			sta zp2
			iny
			lda @FontTabPos,y
			sta zp2+1

		");

		asm("
			ldy #0
			lda #0
ll1:
			sta (p3),y
			sta (p4),y
			iny
			cpy #8
			bne ll1	
		");
		k2_:=sine2[tt+cc]+sx;
		if (tp2[i_]<>$20) then
//		for j_:=0 to 7 do begin
		
/*			k_:=j_+k2_;
			if (k_<8) then 
				p3[k_]:=zp2[j_]
			else
			if (k_<16) then 
				p3[k_-8+8*16]:=zp2[j_];
*/
			asm("

				ldy #0
ppqq:			sty p1
				
				
;				ldy j_
				lda (zp2),y
				sta zp

				tya
				clc
				adc k2_
				tax
				lda tab,x
				tay
				lda zp
				sta (p3),y

				ldy p1
				iny
				cpy #7
				bne ppqq
				
			");
	
/*			k_:=j_+k2_;
			k_:=tab[k_];
			p3[k_]:=zp2[j_];*/
//		end;
		cc:=cc+(sine[time]/8)+16;
		p3:=p3+8;
		p4:=p4+8;
	end;
	//p4[7]:=0;
	poke(^$2000+^128*^8 + ^254,0,0);
//	if (sx=16) then begin
//		sx:=-8;
//	end;
end;


procedure RenderStars();
begin
	moveto(0,@starsY,$D8);
	p1:=screenmemory;
	moveto(0,@starsY,$04);
	k:=0;
	dsx:=time/4;
//	for i:=0 to @starsLines do begin
	for i:=a to b do begin
		for j:=0 to @starsPerLine do begin

			star_dx[k]:=star_dx[k]-star_ddx[k];
			if (star_dx[k]>=127) then begin
				star_dx[k]:=star_dx[x]&7;

				m:=star_x[k];
				l:=screenmemory[m];
		
				if (l>=@starPos and l<@starPosEnd) then
					screenmemory[m]:=$20;
		
				dec(star_x[k]);
		
				if (star_x[k]>=128) then 	
				begin	
					star_x[k]:=39;
					star_ddx[k]:=time&3+1;
				end;
			end;
			
			m:=star_x[k];
			l:=screenmemory[m];
			if (l>=@starPos) then if (l<@starPosEnd) then
				l:=$20;

//			if (l=$20 or (l>@starPos and l<@starPosEnd)) then begin
			if (l=$20) then begin
				p1[m]:=fadeBlue[dsx&15];
				screenmemory[m]:=star_dx[k] + @starPos;
			end;

			inc(k);
			inc(dsx);
		end;
				
		screenmemory := screenmemory + 40;
		p1:=p1+40;
	end;

end;

procedure MoveSprites();


interrupt RasterTop();
begin
	
	StartIRQ(@useKernal);	
/*	call(SIDFILE_1_PLAY);
	CloseIRQ();
	asm(" rti");
*/

	setregularcolormode();
	SCREEN_BG_COL:=bgcol;
	SCREEN_FG_COL:=bgcol;
	i:=sine[time*4]/32;
	scrollx(i);
//		SCREEN_BG_COL:=PURPLE;

@ifdef debugRaster
	SCREEN_BG_COL:=RED;
@endif
//	call(SIDFILE_1_PLAY);
@ifdef debugRaster
	SCREEN_BG_COL:=BLACK;
@endif
//	SCREEN_BG_COL:=BLACK;
	inc(time);
	dscroll:=dscroll+2;
@ifdef debugRaster
	SCREEN_BG_COL:=YELLOW;
@endif
	
//		SCREEN_BG_COL:=RED;
	if (dscroll=8) then begin
		zp:=$0400+40*@ypos;
		p1:=$0400+40*@ypos+1;
		for i:=0 to 4 do begin
			memcpyunroll(p1,0,zp,39);
			zp:=zp+40;
			p1:=p1+40;
		end;
		zp:=$D800+40*@ypos;
		p1:=$D800+40*@ypos+1;
		for i:=0 to 4 do begin
			j:=zp[0];
			memcpy(p1,0,zp,39);
			zp[39]:=j;
			zp:=zp+40;
			p1:=p1+40;
		end;
		dscroll:=0;
//		SetupScrollText();
	end;
	SetupScroll();
@ifdef debugRaster
	SCREEN_BG_COL:=BLACK;
@endif
	
//	SCREEN_BG_COL:=YELLOW;
//	SCREEN_BG_COL:=BLACK;
	if (dscroll<>0) then begin
//		fill(^$2000+^128*^8,0,0);
@ifdef debugRaster
	SCREEN_BG_COL:=BLUE;
@endif
		PrintWaves();
@ifdef debugRaster
	SCREEN_BG_COL:=GREEN;
@endif
		a:=0;
		b:=7;
		RenderStars();


@ifdef debugRaster
	SCREEN_BG_COL:=BLACK;
@endif
/*		zp:=$0400;
		zp2:=$2800;
		k:=sine[time*4]/8;
		if (k<>0) then 
		inczp(zp2,k);
		for j:=0 to 13 do begin
			memcpy(zp2,0,zp,40);
			inczp(zp2,40);
			inczp(zp,40);
		end;
*/
	end;

	y:=142+18; 
	current:=0;
	idx:=0;
//	UpdateRoad();

//	i:=time/2;
//	SPRITE_MULTICOLOR_REG1[1]:=fade2[i&15];


//	RasterIRQWedge(RasterBar(), y,@useKernal);
	RasterIRQ(RasterBar(), y,@useKernal);
	i:=time;
//	colorsRedhues[1]:=fade[i&31];
//	i:=i;
//	colorsRedhues[2]:=fade[i&31];
	hideborderx(1);

	a:=5;
	b:=6;

	if (KeyPressed(KEY_SPACE)=1) then begin
		SetMemoryConfig(1,1,1);
		screenoff();
		asm(" jmp $FCE2 ");
	end;
	CloseIRQ();

end;



interrupt RasterBar();
begin
//	StartIRQWedge(7);
	StartIRQ(@useKernal);
	wait(17);
	SCREEN_BG_COL:=colorsRedhues[idx];
	SCREEN_FG_COL:=SCREEN_BG_COL;
//	j:=idx-cur_start;


//	setmulticolormode();
	inc(idx);


//	shifts[current]:=7-time&7;
	scrollx(shifts[current]);
//	scrollx(0);
	y:=y+16;
	if (idx=2) then y:=y+16;
	inc(current);
//	RasterIRQWedge(RasterBar(), y, @useKernal);
	RasterIRQ(RasterBar(), y, @useKernal);


//	j:=idx-cur_start;
	if (idx=4) then begin // Go to top again
		RasterIRQ(RasterTop(),0,@useKernal);
//		SCREEN_BG_COL:=GREEN;
@ifdef debugRaster
	SCREEN_BG_COL:=PURPLE;
@endif
		if (dscroll=0) then 	begin
			RenderCredzChar();
		end
		else begin
			a:=0;
			b:=8;
			SetupCopyText();	
			CopyText();
		end;
@ifdef debugRaster
	SCREEN_BG_COL:=BLACK;
@endif
//		SCREEN_BG_COL:=BLACK;

	end;
	
	if (idx=2) then
	begin 
		call(SIDFILE_1_PLAY);
		MoveRestSprites();
	end;

	if (idx=1) then 		MoveSprites();


/*	if (idx=3) then begin
		MoveRestSprites();
	end;
*/

/*	if (idx<3) then begin
	a:=3+idx;
	b:=a+1;
	RenderStars();
	end;
*/
//    closeirqwedge();
    closeirq();
end;


procedure SetupSine2();
begin
	for i:=0 to 0 do sine2[i]:=sine[i]/32;

	fill(#tab,254,0);
	for i:=0 to 32 do begin
		if (i<16) then tab[i]:=i+16*8-8;
		if (i<8) then tab[i]:=i;
	end;

end;


procedure InitStars();
begin
	for i:=0 to 24 do begin
		rand(0,160,j);
		star_x[i]:=j/4;	
		star_dx[i]:=random();
		rand(0,255,j);
		star_ddx[i]:=j&3 +1;

	end;
	zp:=$2000+@starPos*8;
	for i:=0 to 8 do begin
		fill(zp,0,8);
		togglebit(zp[3],7-i,1);
		togglebit(zp[4],7-i,1);
		zp:=zp+8;
/*		togglebit(zp[4],8-i,1);
		togglebit(zp[4],6-i,1);
		togglebit(zp[4],7-i,1);
		togglebit(zp[3],7-i,1);
		togglebit(zp[5],7-i,1);*/
	end;
end;


procedure MoveSprites();
begin
	i:=sine[time*2]/4+40;
	int:=i;
	j:=0;
//	poke(^$D010,0,0);
	for i:=0 to 5 do begin
		int:=int+24;
		poke(^$D000,j,int);		

		j:=j+2;
	end;
end;

procedure MoveRestSprites();
begin
	for i:=5 to 8 do begin
		int:=int+24;
		spritepos(int, 210, i);
	end;


end;

procedure InitSprites();
begin
	SPRITE_BITMASK:=$FF;
	SPRITE_MULTICOLOR:=$FF;
	SPRITE_STRETCH_Y:=$FF;
	SPRITE_MULTICOLOR_REG1[0]:=BLUE;
	SPRITE_MULTICOLOR_REG1[1]:=CYAN;
//	fill(^$0800,0,0);
//	fill(^$0900,0,0);
	for i:=0 to 8 do begin
		int:=i*24;
		int:=int+80;
		y:=210;
		spritepos(int,y,i);		
		setspriteloc(i,$A0+i,0);
		SPRITE_COLOR[i]:=PURPLE;
	end;


end;

procedure UpdateRoad();
begin
	road:=(road+1)&15;
	k:=(road+1)&15;
	k:=k*2;
	zp:=$2000+@roadBlock*8;
	j:=road*2;
	zp[6]:=roads[j];
	zp[6+8]:=roads[j+1];
	zp[7]:=roads[k];
	zp[7+8]:=roads[k+1];

end;


procedure InitRoad();
begin
	screenmemory:=$0400+3*40;
	fill(^$2000+^@roadBlock*^8,$FF,16);	
	for i:=0 to 40 do begin
		if (screenmemory[i]=$53) then begin
			screenmemory[i]:=i&1 + @roadBlock;		
		end;
	end;

/*	for i:=0 to 32 do begin
		j:=roads[i];
		asm("
			lda j
			eor #$FF
			sta j
		");
		roads[i]:=j;
	end;*/
end;


procedure InitWaves();
begin
	Screenoff();
	setbank(VIC_BANK0);
//	ClearScreen($20,^$4400);
	ClearScreen($20,^$0400);
/*	i:=peek(^$01,0);
	poke(^$01,0,$33);
	blockmemcpy(^$D000,^$2000,8);
	poke(^$01,0,i);*/
	InitSprites();
//	MULTICOLOR_CHAR_COL[0]:=BROWN;	
	MULTICOLOR_CHAR_COL[2]:=BLACK;	
	MULTICOLOR_CHAR_COL[1]:=RED;	
	hideborderx(1);
	ffld:=100;
	val:=1;
	cur_start:=0;
	decrunch(#logo_col);
	decrunch(#logo_chars);


	tp:=#text;
	InitStars();
	screenmemory:=$0400;
	for i:=0 to 25 do begin
		for j:=0 to 40 do begin
			screenmemory[j]:=screenmemory[j];
		end;
		screenmemory := screenmemory + 40;

	end;

/*	moveto(0,@ypos-2,$D8);
	for i:=0 to 12 do begin
//		j:=(i+3);
		j:=colorsBlues2[i&15];
		fill(screenmemory, j, 40);
		inczp(screenmemory,40);
	end;*/
	initsid(SIDFILE_1_INIT);
	hideborderx(1);
	setcharsetlocation($2000);
	fill(^$2000+^128*^8,0,0);
	tp2:=#waves;
	SetupFontTab();
	SetupSine2();
//	InitRoad();
	fill(^$D800+^14*^40, PURPLE,40);
	fill(^$D800+^15*^40, CYAN,40);
	fill(^$D800+^20*^40, YELLOW,40);
	fill(^$D800+^21*^40, PURPLE,40);

	fill(^$D800+^18*^40, YELLOW,80);

	fill(^$D800+^16*^40, CYAN,80);

	fill(^$0400+^14*^40, $20,160);
	fill(^$0400+^18*^40, $20,160);

	for i:=0 to 105 do begin
		waitforraster(0);
		waitforraster(255);
		call(SIDFILE_1_PLAY);
	end;
	ScreenOn();
end;

procedure PrintWave();
begin

	asm("
		
		ldy varPrefixed_a
pwl:		tya
		adc ms_shift
		and #7
		adc #128
		sta (screenmemory),y
		adc #16
		sta (p1),y
		
		iny
		cpy varPrefixed_b
		bne pwl

	");

/*
	for i:=10 to 30 do begin
		j:=(i+ms_shift)&15;
		screenmemory[i]:=j;
		screenmemory[i+40]:=j+40;

	end;
*/
end;


interrupt nmi();
begin
end;



begin
	preventirq();
	disableciainterrupts();
	nmiirq(nmi());


	SetMemoryConfig(1,@useKernal,0);
	InitWaves();
//	StartRasterChain(RasterTop(),0,@useKernal);
	RasterIRQ(RasterTop(),0,@useKernal);
	
	EnableRasterIRQ();
	enableirq();

	Loop();

end.
